*Area Frequency and Tie-Line Power Control of An Inter-Tied Power System Using – STATCOM*

Prasad Porapu

*Electrical and Electronics Engineering*

*Raghu Engineering College* Visakhapatnam, India

[19985a0263@raghuenggcollege.in](mailto:19985a0263@raghuenggcollege.in)

Anusha Daki   
Assistant professor

Electrical and Electronics Engineering  
*Raghu Engineering College* Visakhapatnam, India  
[daki.anusha92@gmail.com](mailto:daki.anusha92@gmail.com)

Surya Vamsi Rampilla  
*Electrical and Electronics Engineering*  
Raghu Engineering CollegeVisakhapatnam, India  
[suryavamsi.456@gmail.com](mailto:suryavamsi.456@gmail.com)

Sai Srinivas Vurukuti

*Electrical and Electronics Engineering*

Raghu Engineering CollegeVisakhapatnam, India  
[vurukutisaisrinivas@gmail.com](mailto:vurukutisaisrinivas@gmail.com)

Guna Priya Pentakota  
*Electrical and Electronics Engineering*  
Raghu Engineering CollegeVisakhapatnam, India  
[gunapriyapentakota@gmail.com](mailto:gunapriyapentakota@gmail.com)

**Abstract—** **A power system is said to be stable when generation is equal to the demand and unstable due to any uncertainties such as sudden changes in load demand, fault conditions, or any other disturbances; system frequency and voltage will cross its limits. If the system is operating with synchronism, frequency is the main factor needed to be maintained within a permissible limit. This paper demonstrates that single area load frequency control and two-area load and tie-line frequency control and tie-line power damping over the steady-state value can be controlled by a conventional integral controller which makes a steady-state error is zero but it doesn’t show any impact on the transient behavior of the interconnected system concerning load changes. FACTS (Flexible AC Transmission) devices like TCSC and STATCOM Can stimulate the tie-line power oscillations exquisitely under the sudden occurrence of load changes in any of the areas**

Keywords— two areas, tie-line, STATCOM, LFC, AGC

# **Introduction**

The power system is alleged to be perfectly balanced, and stable only if when power generation is capable to the load demand. So, under system balanced criterion; system voltage, frequencies are at their normal operating levels. If load suddenly increases, system fault conditions, disturbances due to system switching, loss of generating unit, failure in the excitation system, failure in turbine governor causes system is to be unstable. If the system operating under unstable or unbalanced condition the system parameters may deviate from its boundaries causes loss in synchronize between control areas. So, we need to control the system parameters under disturbances. One of the main parameters is frequency which shows effect on the power system. A modern power system network is a widely distributed system with a large number of generating stations and load centers. As the load demand on the system for electricity has been increasing day to day, several alternative means of energy productions by using renewable energy resources have gained at most importance. The interaction between generating stations and load demand centers has become very complex due to the injection of renewable energy even at demand centers. Thus, the problem of load frequency control has become a critical issue instability of the power system. Classical control schemes, though proving sufficient operation has many limitations like slow operation, improper tuning of parameters, parametric and non-parametric constraints, damping related issues. For huge-scale power systems involving various interconnected control areas, the main aim is to maintain the system frequency and the tie-line power within the permissible limits. For a similar advantage having Automatic Generation Control (AGC) or Load Frequency Control (LFC) is a very significant FACTS device like static synchronous compensator is one of the basic devices used to reduce harmonics in interconnected power systems. In general, these devices are shunt devices and are connected in parallel with the circuit to control the power system’s steady-state stability and improve transient stability. STATCOM is one of the key controllers that can be founded in two types. One is Voltage Source Controller (VSC) the other one is the Current Source Controller (CSC). Fig. 5 Shows the single line diagram of the STATCOM. In the economical aspect, VSC is mostly used. The main importance of VSC is its output AC voltage can be controlled and leads to reactive power control. A DC-link capacitor acts as a voltage source, and it delivers power as per the converter requirement. Similar to the active filters which absorb harmonics in the system to retain system frequency. Sometimes these STATCOM is also used for injection of current to maintain the system’s active powers within limits.

# **Area load** **— frequency control**

Figure.1 shows the Generic load frequency control mechanism. Changes in load, make variations in the electrical torque of the generator, and this variation results in a mismatch between the mechanical and electrical torque, resulting in speed variations. The governor will sense the variation in speed and adjust the valve position to increase /decrease steam flow from the furnace toward the turbine to balance the torque mismatch (primary loop). This balance is rarely performed at the rated frequency. Therefore, “to achieve the rated frequency of the system and recompense for power imbalance”, the governor’s set point is changed by the actions of an automatic load frequency control controller whose decisions are taken promptly and have to offer a strong power system operation under several contingency situations.



Figure1. Generic load frequency scheme

## **Single-area load frequency control**

A single control area is nothing but an area in which all the generators are closely coupled together, synchronized to control the output power of all the generators to maintain the scheduled frequency of the system within a permissible limit. In such an electric area all the generators whose speeds increasing and decreasing simultaneously in such a coherent area can be called a control area. During both dynamic and static conditions the frequency response is the same.

A single control area consisting of a turbine, governor, electric generators whose transfer functions are indicated in the block diagram as shown in Figure.2, where Ki is the integral controller gain constant, ,, are the governor, turbine, generator gain constants, Ad, , the governor, turbine, generator time constants. And is the deviation in load demand be the change in area Frequency concerning load change.




Figure 2. Single area load frequency control block diagram

## **Load frequency control — single area**

Figure.3 indicates the frequency response of the single area load-frequency control. The steady-state frequency deviations due to change in two parameters one is change in load other one is change in speed changer setting. In this the main objective of the speed changer setting is to bring the steady state system frequency to the scheduled frequency by adjusting itself when the system subjected to unacceptable dynamic system frequency deviations. When there is a sudden change in load then speed changer setting can be automatically adjusted by observing the changes is frequency. A signal can be feedback to input through integrator to the speed changer. Now the system can be modified into proportional plus integral controller which gives steady state error to be zero.




Figure 3. Single control area load frequency response

## **Load frequency control — Two area**

A number of control areas are when interconnected forms a large power system. In case of two, single control areas are inter-tied there may be deviation in the entire system frequency need to be control knows as two area load frequency control and, are inter-tied by line called tie-line whose frequency, tie line power are need to be constant under normal operating conditions. If any one of area load changes suddenly, entire power system frequency and tie line power also changes. Fig.4 shows interconnected system block diagram.





Figure 4. Single line diagram of interconnected system

# **Formulation**



From Area 1, to Area 2 change in tie line power

🡪(1)

From Area 2, to Area 1 change in tie line power

🡪(2)

# **Controller**

**STATCOM:**

Static synchronous compensator (SATCOM), or it is also known as a static synchronous generator can be operated as static VAR compensator connected in parallel, whose capacitive and inductive output currents can control which are not dependent of a system voltage (AC)




Figure 5. STATCOM single line diagram

Figure.6 indicates that simple operating principle of STATCOM which is connected in shunt to the power line through the magnetic circuit. In general, STATCOM’s are operated with power electronics devices. From the figure Iq and Es be the STATCOM current and voltage, Idc, Vdc are the capacitor current and voltages. And Et be the utility terminal voltage. If Es>Et it supplies reactive power and Es<Et it absorbs reactive power.




Figure 6. simple operating principle

1. **System Parameters**

|  |  |
| --- | --- |
| Ki (integrator gain constant) | 0.09 |
| Ksg (governor gain constant) | 100 |
| Kt (turbine gain constant) | 1 |
| Kps (generator gain constant) | 1 |
| R(speed regulator constant) | 3 |
| B(biasing coefficient) | 0.425 |
| ΔPd (percentage change in load) | 1% |
| Tsg (governor time constant) | 0.4 |
| Tt (turbine time constant) | 0.5 |
| Tps (generator time constant) | 20 |
| T12, T21 (synchronizing coefficient) | 1 |

# **Simulation results**

## **Two area load frequency control without controller**

Simulation block diagram of two area load frequency control, designed in simulation using Figure.3 and run the simulation in MATLAB with the help of parameters provided in table.1.and, the simulation gives the results for change in frequency and tie line power with the change in load. Figure.6 indicates the two-area load frequency control without any controller with the 10 % change(increase) in load in area.1 shows the effect not only on the frequency of area.1 but also it shows the impact on area.2 frequency and tie line power. there is some instability in both transient and steady state frequency response of area 1,2 and tie line power Ptie 1,2. Figure.7 shows the tie-line power having a greater number of oscillations due to sudden change in load


****

Figure 7. Two area load frequency without controller


****

Figure 8. Tie-line power without controller

## **Two-area load frequency control with integral controller**

The main application of controller with integral controller is to bettering the steady – state response. In integral controller as Ki value increases the magnitude also increases and due to pole at origin which makes steady state error equals to zero. Figure.8 indicates two-area interconnected system frequency response. System whose steady state error makes to zero even with sudden increase in load to 10% and Figure.9 shows the tie-line power of interconnected system whose oscillations can be reduced about its final equilibrium point.




Figure 9. Two area load frequency control with integral controller




Figure 10. Two - area load frequency control, tie line power with integral controller

## **Two-area load frequency control with STATCOM controller**

Integral controller only improves the steady state response ,but it doesn’t show any effect on the transient response. And the STATCOM is used to improve both the transient response and inject the reactive power and absorbs so that it reduces the power oscillation damping’s of the tie-line power with sudden change in load. Figure.11 shows the two-area load frequency control with STATCOM reduce both steady state error to zero and Figure.12 shows two-area load frequency control tie line power with STATCOM which reduce the both steady state and transient oscillations tie-line power.




Figure 11. Two area load frequency control with STATCOM controller




Figure 12. Two - area load frequency control, tie line power with STATCOM

##### **Conclusion**

In this paper, two area load frequency control was modelled using MATLAB simulation for controlling area load frequency and tie line power which changes due to sudden change(increase) in load. Integral controller is used to improve the steady state response which makes steady state error is equals to zero and to improves the damping oscillations in tie line power the best controllers are FACTS devices. STATCOM is one of the basic FACTS device which is connected in series to the tie line to make the steady state error to zero and reduce the tie line power oscillation in transient state.

##### **References**

1. Kundur P.: ”Power stability and control”, Mcgraw Hill, 2009
2. Concordia, C., & Kirchmayer, L. K. (1954). Tie-Line Power and Frequency Control of Electric Power Systems - Part II [includes discussion]. Transactions of the American Institute of Electrical Engineers. Part III: Power Apparatus and Systems, 73(2), 133–146.
3. Kirchmayer, L.K: Economic control of interconnected systems. (1960). Journal of the Franklin Institute, 269(6), 492–493.
4. Jaleeli, N., VanSlyck, L. S., Ewart, D. N., Fink, L. H., & Hoffmann, A. G. (1992). Understanding automatic generation control. IEEE Transactions on Power Systems, 7(3), 1106–1122.
5. Das, D., Kothari, M. L., Kothari, D. P., & Nanda, J. (1991). Variable structure control strategy to automatic generation control of interconnected reheat thermal system. IEE Proceedings D Control Theory and Applications, 138(6), 579.
6. Chan, W.-C., & Hsu, Y.-Y. (1981). Automatic generation control of interconnected power systems using variable-structure controllers. IEE Proceedings C Generation, Transmission and Distribution, 128(5), 269.
7. Pal, B. C., Coonick, A. H., & Macdonald, D. C. (n.d.). Robust damping controller design in power systems with superconducting magnetic energy storage devices. 2000 IEEE Power Engineering Society Winter Meeting. Conference Proceedings (Cat. No.00CH37077).
8. Abraham, R. J., Das, D., & Patra, A. (2007). Effect of TCPS on oscillations in tie-power and area frequencies in an interconnected hydrothermal power system. IET Generation, Transmission & Distribution, 1(4), 632.
9. Bikash Pal and Balarko Chaudhuri. Robust Control in Power Systems. (2005). Power Electronics and Power Systems.
10. Hingorani,N.G and Gyugi,L.:”Understanding FACTS” (IEEE Press,2000)
11. Pal,B.C, Rehantz,C. and Zhang, X.P:”Flexible AC Transmission Systems: Modelling and Control”,(Springer,2006)
12. Kimbark, E.W:”Improvement of System stability by switched series capacitors”,IEEE Trans. Power Apparatus Syst. 1966,PAS-85,(2), pp.180-188
13. Rajaraman et al, Computing the damping of sub-synchronous oscillations due to a TCSC, IEEE Trans on Power Del,Vol.11,No.2,April 1996.
14. Jonas Persson, Lennart Soder:”Validity of a linear Model of a thyristor-controlled series capacitor for Dynamic Simulations”, in Proc.14th Power Systems Computation Conference, June 24th - 28th,2002,Sevilla,Spain.
15. P. Mattavelli,G.C Verghese,A.M Stankovic,”Phasor dynamics of Thyristor Controlled Series Capacitor Systems”,IEEE Summer Meeting 532-2 PWRS,1996.
16. H.A.Othman, L.Angquist, et al.,:”Analytical Modeling of Thyristor- Controlled Series Capacitors for SSR studies”,IEEE Trans. Power Systems,Vol.11,No.1,1996,pp.119-127.
17. John J Paserba,Nicholas W.Miller et al,”A thyristor Controlled Series Compensation Model for Power System Stability Analysis”,IEEE Trans.Power Delivery,Vol.10,No.3,1995,pp.1471-1478.
18. Saadat,H.:”Power System Analysis”, McGraw Hill,USA,1999.
19. Ibraheem, Prabhat Kumar and D. P. Kothari “Recent Philosophies of Automatic Generation Control Strategies in Power Systems”, IEEE Trans. on Power System, Vol. 20, No.1, pp. 346-357, Feb 2005.
20. K. C. Divya and P. S. N. Rao, “A Simulation Model for AGC Studies of Hydro-Hydro Systems” Electrical Power and Energy Systems 27, pp.335-342, 2005
21. R.J. Abraham, D.Das and A.Patra: “AGC study of a Hydrothermal system with SMES and TCPS”, European Transactions on Elecrical Power, Vol.19, pp.487-498, April 2009.
22. IEEE Committee Report: ‘Dynamic models for steam and hydro turbines in power system studies’, IEEE Trans. Power Appar. Syst., 1973, 92, (6), pp. 1904– 1915.
23. Control and analysis of Multi terminal HVDC Grid published in IJAEMA, UGC indexed ISSN 0886-9367, vol-12,issue-01,2020.
24. Design and Implementation of Women safety system based on IoT technology.
25. A New Three-phase Advanced Level VSI Published in IJRTE, SCOPUS indexed ISSN 2319-8885, VOL-6, issue-32, pages-6464-6467,2017.
26. N. Cohn, Control of Generation and Power Flow on Interconnected Systems, New York, John Wiley,1986.